

Micing
======

Mic was positioned in the following locations:

                              __       __
                             / |\_____/  \                                        
                            /  |          \
                           /   D           \
                          /                 \
                         / |               / \
                        /  E              C   \
                    ___/                     / \___
                                            B  | 
                                               |
                                               A                                                

A = Edge straight on
B = Edge angle
C = Cone mid
D = Voice coil edge
E = Cone straight


Files are names by speaker type, followed by a number giving the approximate location:

0.  Edge straight on, 1" from cone
1.  Edge straight on, 2"
2.  Edge angle, 1"
3.  Edge angle, 2"
4.  Cone mid, 1"
5.  Cone mid, 2"
6.  Cone mid, 3"
7.  Cone mid, 5"
8.  Cone mid, 8"
9.  Cone mid, 12"
10. Voice coil edge, 2"
11. Voice coil edge, 3"
12. Voice coil edge, 5"
13. Cone straight, 1"
14. Cone straight, 2"
15. Cone straight, 3"
16. Cone straight, 4"

With the speakers on the (hard wood) floor, I miked from two other positions:

15.  Mic about 2' away, pointing at the floor between the cab and speaker (pick up reflections 
     off floor)
16.  Mic about 2' away, resting on floor

In one or two cases, I accidentally ommitted a position, so the numbers may not track 100% 
perfectly....



Good starting positions are #12/#13/#14.

