01
Amp: 5150 Loop In
Cab: V4 4x12
Speaker: v30 Top Right
Mics: i5 Straight on / 421II @ 45 deg
File: 01a_v4-4x12-v30_i5-421.wav

02
Amp: 5150 Loop In
Cab: Cobra 4x12
Speaker: Greenback Top Right
Mics: i5 Straight on / 421II @ 45 deg
File: 02a_cob-4x12_gb_i5-421.wav

03
Amp: 5150 Loop In
Cab: Mesa 2x12
Speaker: gs1275
Mics: i5 Straight on / 421II @ 45 deg
File: 03a_mes-2x12-gs1275_i5-421.wav

04
Amp: 5150 Loop In
Cab: Mesa 2x12
Speaker: v30
Mics: i5 Straight on / 421II @ 45 deg
File: 04a_mes-2x12-v30_i5-421.wav

05
Amp: Dual Rectifier Loop In
Cab: Mesa 2x12
Speaker: v30
Mics: i5 Straight on / 421II @ 45 deg
File: 05a_mes-2x12-v30_i5-421.wav

06 
Amp: 5150 Loop In
Cab: V4 4x12
Speaker: v30 Top Left
Mics: 57 straight on / 421II @ 45 deg
File: 06a_v4-4x12-v30_57-421.wav

07
Amp: 5150 Loop In
Cab: V4 4x12
Speaker: v30 Top Left
Mics: 57 straight on / 421II @ 45 deg
File: 07a_v4-4x12-v30_57-421.wav

08
Amp: 5150 Loop In
Cab: V4 4x12
Speaker: v30 Top Left
Mics: 57 no xfmr straight on / 421II @ 45 deg
Same as 07 but mics moved some to the right
File: 08a_v4-4x12-v30_57nx-421.wav

09
Amp: 5150 Loop In
Cab: Cobra 4x12
Speaker: Greenback Top Left
Mics: 57 straight on / 421II @ 45 deg
File: 09a_cob-4x12-gb_57-421.wav

10
Amp: 5150 Loop In
Cab: Mesa 2x12
Speaker: v30
Mics: 57 straight on / 421II @ 45 deg
File: 10a_mes-2x12-v30_57-421.wav

11
Amp: 5150 Loop In
Cab: Mesa 2x12
Speaker: v30
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 11a_mes-2x12-v30_ 57nx-421.wav

12
Amp: 5150 Loop In
Cab: Mesa 2x12
Speaker: gs1275
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 12a_mes-2x12-gs1275_57nx-421.wav

13
Amp: 5150 Loop In
Cab: Mesa 2x12
Speaker: gs1275
Mics: 57 straight on / 421II @ 45 deg
File: 13a-mes-2x12-gs1275_57-421.wav

14
Amp: 5150 Loop In
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 14a-v4-4x12-v30_57nx-421.wav

15
Amp: 5150 Loop In
Cab: cobra 4x12
Speaker: greenback
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 15a-cob-4x12-gb_57nx-421_32.wav

16
Amp: 5150 Loop In
Cab: mesa 2x12
Speaker: gs1275
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 16a-mes-2x12-gs1275_57nx-421_32.wav

17
Amp: 5150 Loop In
Cab: mesa 2x12
Speaker: v30
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 17a-mes-2x12-v30_57nx-421.wav

18
Amp: 5150 Loop In
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 18a-mes-2x12-v30_57nx-421.wav
 
19 to 21 used the 5150 Rhythm Channel with varying degrees of drive
Amp: 5150
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / i5 @ 45 deg
File: 19a-v4-4x12-v30_57nx-i5.wav
File: 20a-v4-4x12-v30_57nx-i5.wav
File: 21a-v4-4x12-v30_57nx-i5.wav

22 to 24 used the 5150 Effects Return Input with varying degrees of Presence Resonance = ~7
Amp: 5150
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / i5 @ 45 deg
File: 22a-v4-4x12-v30_57nx-i5.wav
File: 23a-v4-4x12-v30_57nx-i5.wav
File: 24a-v4-4x12-v30_57nx-i5.wav

25 to 27 used the 5150 Effects Return Input with varying degrees of Resonance Presence = ~9
Amp: 5150
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / i5 @ 45 deg
File: 25a-v4-4x12-v30_57nx-i5.wav
File: 26a-v4-4x12-v30_57nx-i5.wav
File: 27a-v4-4x12-v30_57nx-i5.wav
 
28 to 30 used the 5150 Effects Return Input with varying degrees of Resonance Presence Resonance = ~7
Amp: 5150
Cab: Cobra 4x12 Top Left
Speaker: Greenback
Mics: 57 no xfmr straight on / i5 @ 45 deg
File: 28a-cob-4x12-gb_57nx-i5.wav
File: 29a-cob-4x12-gb_57nx-i5.wav
File: 30a-cob-4x12-gb_57nx-i5.wav

31 to 33 used the 5150 Effects Return Input with varying degrees of Resonance Presence = ~9
Amp: 5150
Cab: Cobra 4x12 Top Left
Speaker: Greenback
Mics: 57 no xfmr straight on / i5 @ 45 deg
File: 31a-cob-4x12-gb_57nx-i5.wav
File: 32a-cob-4x12-gb_57nx-i5.wav
File: 33a-cob-4x12-gb_57nx-i5.wav

34 using 24a-v4-4x12-v30_57nx-i5.wav filtered with CurveEQ using Impulse 24d against Unearth's Sanctity of Brother
Amp: 5150
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / i5 @ 45 deg
File: 34a-v4-4x12-v30_57nx-i5.wav

35 using 24a-v4-4x12-v30_57nx-i5.wav filtered with CurveEQ using Impulse 24a against Unearth's Sanctity of Brother
Amp: 5150
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / i5 @ 45 deg
File: 35a-v4-4x12-v30_57nx-i5.wav

36
Amp: 5150 Loop In
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 36a-mes-2x12-v30_57nx-421.wav

37
Amp: Cobra Effects Return Deep @ 12:00
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 37a-mes-2x12-v30_57nx-421.wav

38
Amp: Cobra Effects Return  Deep @ 3:00
Cab: v4 4x12
Speaker: v30
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 38a-mes-2x12-v30_57nx-421.wav

39-43
Amp: Cobra Effects Return  Deep @ 3:00 (Mike's Cab)
Cab: Splawn 4x12
Speaker: Govenor (Top Left)
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 39a-spln-4x12-gvnr_57nx-i5_32.wav
File: 40a-spln-4x12-gvnr_57nx-i5_32.wav
File: 41a-spln-4x12-gvnr_57nx-i5_32.wav
File: 42a-spln-4x12-gvnr_57nx-i5_32.wav
File: 43a-spln-4x12-gvnr_57nx-i5_32.wav

44-48
Amp: Cobra Effects Return  Deep @ 3:00 (Mike's Cab)
Cab: Splawn 4x12
Speaker: Manowar (Top Right)
Mics: 57 no xfmr straight on / 421II @ 45 deg
File: 44a-spln-4x12-gvnr_57nx-i5_32.wav
File: 45a-spln-4x12-gvnr_57nx-i5_32.wav
File: 46a-spln-4x12-gvnr_57nx-i5_32.wav
File: 47a-spln-4x12-gvnr_57nx-i5_32.wav
File: 48a-spln-4x12-gvnr_57nx-i5_32.wav

49-52
Amp: 5150 Effects Return  Resonance: 7  Presence: 9
Cab: Cobra 4x12
Speaker: Greenback (Top Right)
Mics: 57 with 680 ohm load cable straight on / 57 no xfmr @ ~15 deg
File: 49a-cob-4x12-gb_57-57nx
File: 50a-cob-4x12-gb_57-57nx
File: 51a-cob-4x12-gb_57-57nx
File: 52a-cob-4x12-gb_57-57nx

53-56
Amp: 5150 Effects Return  Resonance: 7  Presence: 9
Cab: V4 4x12
Speaker: V30 (Top Right)
Mics: 57 with 680 ohm load cable straight on / 57 no xfmr @ ~15 deg
File: 53a-cob-4x12-gb_57-57nx
File: 54a-cob-4x12-gb_57-57nx
File: 55a-cob-4x12-gb_57-57nx
File: 56a-cob-4x12-gb_57-57nx

57-60
Amp: 5150 Effects Return  Resonance: 7  Presence: 9
Cab: Cobra 4x12
Speaker: gs1275
Mics: 57 with 680 ohm load cable straight on / 57 no xfmr @ ~15 deg
File: 57a-cob-4x12-gb_57-57nx
File: 58a-cob-4x12-gb_57-57nx
File: 59a-cob-4x12-gb_57-57nx
File: 60a-cob-4x12-gb_57-57nx

